22.11.2004, FS FORTH-SYSTEME GmbH

This run time version of the "Kithara DOS Enabler, Version 6.04d" 
is configured to give support for some of our DOS based tools 
for WinNT, Windows2000 and WindowsXP. After installation of the "DOS Enabler" 
the accesses to the LPT ports are allowed for the 
programms listed below.

Note1: Accesses to the ports are only allowed for the programms listed 
       below. If you rename one of our tools, the DOS Enabler does not work. 

Note2: Under Windows NT, Windows 2000 and Windows XP you must use the option 
       /LPT-BASE=378 (for JTAG-Booster) to get access to the standard 
       parallel port. 

This run time installation of Kithara 6.x 
is configured for the following DOS programs:

Program name  : Description                            : used ports
--------------: ---------------------------------------:-----------
JTAG386.exe   : JTAG-Booster for Intel 386EX           : LPT1+LPT2
JTAGEL4.exe   : JTAG-Booster for AMD ElanSC400/410     : LPT1+LPT2
JTAGEL5.exe   : JTAG-Booster for AMD ElanSC520         : LPT1+LPT2
JTAG060.exe   : JTAG-Booster for ADSP-21060/21061/21062: LPT1+LPT2
JTAG065.exe   : JTAG-Booster for ADSP-21065            : LPT1+LPT2
JTAG161.exe   : JTAG-Booster for ADSP-21161            : LPT1+LPT2
JTAG823.exe   : JTAG-Booster for Motorola MPC823       : LPT1+LPT2
JTAG860.exe   : JTAG-Booster for Motorola MPC860       : LPT1+LPT2
JTAG8260.exe  : JTAG-Booster for Motorola MPC8260      : LPT1+LPT2
JTAG120.exe   : JTAG-Booster for Galileo 64120         : LPT1+LPT2
JTAG1200.exe  : JTAG-Booster for National Geode SC1200 : LPT1+LPT2
JTAGARM7.exe  : JTAG-Booster for ARM7TDMI              : LPT1+LPT2
JTAGARM9.exe  : JTAG-Booster for ARM9                  : LPT1+LPT2
JTAG7520.exe  : JTAG-Booster for NetSilicon NS7520     : LPT1+LPT2
JTAG9750.exe  : JTAG-Booster for NetSilicon NS9750     : LPT1+LPT2
JTAG9360.exe  : JTAG-Booster for NetSilicon NS9360     : LPT1+LPT2
JTAG1100.exe  : JTAG-Booster for Intel SA-1100         : LPT1+LPT2
JTAG1110.exe  : JTAG-Booster for Intel SA-1110         : LPT1+LPT2
JTAG250.exe   : JTAG-Booster for Intel PXA210/250      : LPT1+LPT2
JTAG255.exe   : JTAG-Booster for Intel PXA255/26x      : LPT1+LPT2
JTAG270.exe   : JTAG-Booster for Intel PXA27x          : LPT1+LPT2
JTAG321.exe   : JTAG-Booster for Intel IOP321          : LPT1+LPT2
JTAG425.exe   : JTAG-Booster for Intel IXP425          : LPT1+LPT2
JTAG2410.exe  : JTAG-Booster for Samsung S3C2410       : LPT1+LPT2
JTAG2440.exe  : JTAG-Booster for Samsung S3C2440       : LPT1+LPT2
JT405EP.exe   : JTAG-Booster for IBM PPC405EP          : LPT1+LPT2
JT405GP.exe   : JTAG-Booster for IBM PPC405GP          : LPT1+LPT2
JT405GPR.exe  : JTAG-Booster for IBM PPC405GPr         : LPT1+LPT2
JT440GP.exe   : JTAG-Booster for IBM PPC440EP          : LPT1+LPT2
JTAu1000.exe  : JTAG-Booster for AMD Alchemy Au1000    : LPT1+LPT2
JTAu1100.exe  : JTAG-Booster for AMD Alchemy Au1100    : LPT1+LPT2
JTAu1500.exe  : JTAG-Booster for AMD Alchemy Au1500    : LPT1+LPT2
JTAu1550.exe  : JTAG-Booster for AMD Alchemy Au1550    : LPT1+LPT2
JTAGE400.exe  : JTAG-Booster for Siemens ERTEC400      : LPT1+LPT2
JTAGE200.exe  : JTAG-Booster for Siemens ERTEC400      : LPT1+LPT2
JTAGF020.exe  : JTAG-Booster for Cygnal C8051F02x/F12x : LPT1+LPT2

REMHOST.exe   : Remote Server for Insyde BIOS          : LPT1+LPT2
EXPRESS.exe   : Lattice PLD programmer                 : LPT1+LPT2


Installation:
=============

Important: You need administrator rights to install this program!!


1. Installation on a clean system (no previous version of Kithara installed) 
----------------------------------------------------------------------------

If you have a clean system without having installed a previous version of 
the "Kithara Tool Center", this tool is really simple to install. 
Extract the ZIP file to a new folder and start KSETUP.EXE. 
Everything is done within a few seconds. No additional input is needed.
Now reboot your PC.


2. Installation, if you have already installed a version 5.x/6.x of Kithara Tool 
--------------------------------------------------------------------------------

If you have already installed an older WinNT support (Kithara Version 5.x or 6.x), 
you have to de-install it first as described below.

After rebooting your PC you can install the Kithara 6.x as described above.


3. Installation, if you have already installed a version 4.x of Kithara Tool 
----------------------------------------------------------------------------

Important!! If you have already installed an older WinNT support, you 
have to deinstall it completely!!!

- Start kcenter
- Select Register "Einstellungen" (=Settings) 
  and deactivate "VDD benutzen" 
  and "speziellen seriellen Treiber benutzen".
- Stop Kernel
- exit the kcenter program
- Now you can deinstall the Kithara Package with: 
  Settings - Control Panel. 
  All unused parts must be removed.
- Reboot your PC
- Now you can install the Kithara 6.x as described above.


De-Installation version 6.x:
=============================

Important: You need administrator rights to de-install this program!!

For de-installation of the runtime version of the 
"Kithara DOS-Enabler Version 6.x":

- use: Settings - Control-Panel - Add/Remove Programs
  and remove the
  "FS FORTH-SYSTEME WinNT Support"

- Reboot your PC


