Digi JumpStart™
for Windows Embedded Compact 7 Feature Pack 1

Release Notes 
Build 1.0.0.1
03 August, 2011

© 2011, Digi International
http://www.digiembedded.com

Introduction
This document provides information about the Digi JumpStart™ Kit Feature Pack for Windows Embedded Compact 7, for the ConnectCore™ family of embedded modules.
Contents
This document contains these sections:
1.	Supported Platforms
2.	Features
3.	Fixes and improvements 
5.	Known Issues and Limitations
5.	Support Contact Information

1.	Supported Platforms
The BSP supports following hardware platforms:

·    ConnectCore™ i.MX51 (PN CC-MX51-CE7) 
·	ConnectCore™ Wi-i.MX51 (PN CC-WMX51-CE7)		 

2.	Features
2.1 Installer
Easy installation process that allows backup the previous installed sources:

·	New features for Digi JumpStart™ Kits
•	Update BSP version to v3.1

2.2 New features
·	No new features included

2.3 Support for new module variants (i.MX51 only)
Here the list of additional variants that are support now.

·	55001585-02
•	55001585-03
•	55001585-05
•	55001445-03
•	55001445-04
•	55001445-06
3.	Fixes and Improvements
3.1 Fixes
	·	Fixed NVRAM bad block detection
·	Fixed i.MX51 serial baud rate calculation
·	Fixed problems with wireless driver (RedPine) when more than 40 AP are detected.

3.2 Enhancements
·	Wi-Fi driver update for CC-WMX51-CE7 to version 3.2.7b.
4.	Known Issues and Limitations
·	No known issues detected in this Feature Pack.   
5.	Support Contact Information
For any technical support related questions about your development kit, please contact the Digi technical support experts:

·	Digi Technical Support Web Site
http://www.digi.com/support/index.jsp
·	Online Support Forum
http://www.digi.com/support/forum/
·	Online submission of questions/issues
http://www.digi.com/support/eservice/login.jsp